{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["HK-D01"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":137,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"HK-D01","index":0,"n_rows":45,"n_cols":18,"rows_kept":45,"cut":false,"hidden":false,"merged":[[11,11,11,16],[5,11,5,16],[0,0,0,9],[0,11,0,16]]}
["LOPEZ LABS EMISSIONS TEST DATA FORM",null,null,null,null,null,null,null,null,null,null,"DATA INPUT SCREEN:"]
["Revised Jan 16/09"]
["RUN No.",null,{"$f":"RunNumber","v":"HKK-12"},null,"Heater ID",{"$f":"Q8","v":"HK"},null,"DATE",null,{"$f":"DATE","v":"2009-01-19"},null,"Instructions:",null,"Enter data only into fields that are"]
["Wood Moisture %",null,{"$f":"AVERAGE(Moisture)","v":20},null,"Time since last burn",null,{"$f":"TimeSinceLast","v":24},"Ambient Temperature",null,{"$f":"AmbientTemperature","v":0},null,null,null,"shaded like this box"]
["Total Weight lbs",null,{"$f":"SUM(PcWt)+WtKindl-UnburnedFuel","v":62.95},null,"Start Time",null,{"$f":"(StartTime)","v":"14:15:00"},null,null,null,null,null,null,"Slide graph over when done and start test"]
["Kindling Weight lbs",null,{"$f":"KindlingWeight","v":4.5},null,"FUELING",null,null,null,null,null,null,"GENERAL"]
["Number of Pieces",null,{"$f":"COUNT(PcWt)","v":7},null,"Fuel Type..........................",null,null,{"$f":"FuelType","v":"Wh. Birch"},null,null,null,"RUN No.",null,"HKK-12","DATE",null,"2009-01-19"]
["Fuel Surface/Vol",null,{"$f":"(AVERAGE(Length)+SUM(Circumf))/(WtFuel-WtKindl)","v":{"$error":"#DIV/0!"}},null,"Fuel Density......................",null,null,{"$f":"O15","v":"smaller towards top"},null,null,null,"Time since last burn",null,24,"HEATER ID",null,"HK"]
["Average Pc. Wt. lbs",null,{"$f":"AVERAGE(PcWt)","v":8.35},null,"Unburned Fuel.................",null,{"$f":"UnFuel","v":0},{"$f":"UnFuel","v":0},null,null,null,"Start Time",null,"14:15:00","Ambient Temperature"]
["Run Length hrs",null,1.9,null,null,null,null,null,null,null,null,null,null,null,"Weather"]
["Av. Stack Temp F",null,{"$f":"AVERAGE(StackTemp)","v":361}]
["Av. O2%",null,{"$f":"G14","v":13.82},null,"GAS DATA FROM TESTO SPREADSHEET",null,null,null,null,null,null,"FUELING"]
["Av. CO%",null,{"$f":"AVERAGE(CO)/10000","v":6.6810000000000008E-2},null,null,"StackTemp","O2% x10","ppm CO",null,null,null,null,null,null,"Fuel Configuration:"]
["Stack Temp Factor",null,{"$f":"SQRT(528/(460+AvStackTemp))","v":0.801946474896716},null,null,361,13.82,668.1,null,null,null,"Fuel Type",null,"Wh. Birch",222]
["Stack Dilution Factor",null,{"$f":"20.9/(20.9-_AvO2)","v":2.9519774011299442},null,null,null,null,null,null,null,null,null,null,null,"smaller towards top"]
["Burn Rate  dry kg/hr",null,{"$f":"((WtFuel-(UnburnedFuel*(1+AvMoisture/100)))/RunLength)*(1-(AvMoisture/100))/2.2","v":12.047846889952154},null,null,null,null,null,null,null,null,"Kindling Weight",null,4.5]
["Boiling of Water Loss",null,{"$f":"(8.05+0.0035*(AvStackTemp-70))+(2.58+0.00114*AvStackTemp)","v":12.060040000000001},null,null,null,null,null,null,null,null,"Unburned Fuel",null,0]
["CO Loss %",null,{"$f":"gmKgCO*9.75/86","v":1.3259140053458816}]
["HC Loss %",null,{"$f":"gmKgCondar*33/86","v":0.34012583183876027}]
["Dry Gas Loss %",null,{"$f":"((1.5*DilutionFactor*(AvStackTemp-70))/8600)*100","v":14.983001576665355},null,null,null,null,null,null,null,null,null,"DETAILED FUEL INFORMATION"]
["Filter Catch gm",null,{"$f":" Catch","v":6.0200000000000031E-2},null,null,null,null,null,null,null,null,null,"Piece #","Weight","Moisture","Circumf","Length","Shape"]
["g/kg    Condar",null,{"$f":"(Catch/RunLength)*3.04*(DilutionFactor)/(0.4*StackTempFactor)","v":0.88638853145858743},null,null,null,null,null,null,null,null,null,1,10.6,20,null,null,5]
["g/kg    CO",null,{"$f":"59.3*AvCO*DilutionFactor","v":11.695241483050852},null,null,null,null,null,null,null,null,null,2,9.75,20,null,null,2]
["Combustion Effic",null,{"$f":"100-COLoss-HCLoss","v":98.333960162815359},null,null,null,null,null,null,null,null,null,3,8.6999999999999993,20,null,null,2]
["Heat Trans. Effic",null,{"$f":"100-DryGasLoss-BoilWaterLoss","v":72.95695842333464},null,null,null,null,null,null,null,null,null,4,8.6,20,null,null,2]
["Overall Efficiency",null,{"$f":"HTransEffic*CombustEffic/100","v":71.741466432003648},null,null,null,null,null,null,null,null,null,5,8.3000000000000007,20,null,null,2]
["Filter","Clean","Dirty","Wt. of",null,null,null,null,null,null,null,null,6,6.6,20,null,null,3]
["Number","Filter Wt.","Filter Wt.","Particulat",null,null,null,null,null,null,null,null,7,5.9,20,null,null,2]
[1,1.0088999999999999,1.0669999999999999,{"$f":"IF(FiltDirty-FiltClean>0,FiltDirty-FiltClean,0)","v":5.8100000000000041E-2},null,null,null,null,null,null,null,null,8]
[2,1.0106999999999999,1.0127999999999999,2.0999999999999908E-3,null,null,null,null,null,null,null,null,9]
[3,null,null,0,null,null,null,null,null,null,null,null,10]
[4,null,null,0,null,null,null,null,null,null,null,null,11]
[5,null,null,0,null,null,null,null,null,null,null,null,12]
[6,null,null,0,null,null,null,null,null,null,null,null,13]
["Ctrl 1",0,0,null,null,null,null,null,null,null,null,null,14]
["Ctrl 2",0,0,null,null,null,null,null,null,null,null,null,15]
[null,"Adjust",null,{"$f":"+COUNT(FiltClean)*(AVERAGE(CleanControl)-AVERAGE(DirtyControl))","v":0},null,null,null,null,null,null,null,null,16]
[null,"Total",null,{"$f":"SUM(D29:D34)+D37","v":6.0200000000000031E-2},null,null,null,null,null,null,null,null,17]
[null,null,null,null,null,null,null,null,null,null,null,null,18]
[null,null,null,null,null,null,null,null,null,null,null,null,19]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Shape key:",null,1,"round"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"half"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"quarter"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"smaller than quarter"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"other"]